## --node SMA
SMA
  in   series:F64
  out  value:F64
  param length:I64  (bind {"I64": <v>})
[exit=0]

## --node Sub
Sub
  in   lhs:F64
  in   rhs:F64
  out  value:F64
[exit=0]

## --node Bias
Bias
  in   signal:F64
  out  bias:F64
  param scale:F64  (bind {"F64": <v>})
[exit=0]

## --node EMA
EMA
  in   series:F64
  out  value:F64
  param length:I64  (bind {"I64": <v>})
[exit=0]

## --node RollingMax
RollingMax
  in   series:F64
  out  value:F64
  param length:I64  (bind {"I64": <v>})
[exit=0]

## --node LinComb
aura: unknown node type "LinComb"
[exit=2]

## --node Recorder
aura: unknown node type "Recorder"
[exit=2]

